**ABSTRACT**

The intensity distribution in the focal region of a high NA lens for the incident azimuthally polarized Laguerre Bessel Gaussian beam (LBG) transmitted through a multi belt spiral phase hologram (MBSPH) is studied on the basis of the vector diffraction theory. Here we report a new method that generates a multiple transversely polarized focal spots suitable for multilayer optical recording and multiple optical trapping.