**ABSTRACT**

Polyvinylidene fluoride (PVDF) and Trifluoroethylene ((TrFE) are potential polymers which are used in acoustic transducers and electromechanical actuators because of their inherent piezoelectric response, as heat sensors because of their inherent pyroelectric response and as dielectric layer in organic thin film.